**PO2EBL\_ELECTRIC BLENDER**

**GDD DOCUMENT**

**Version 1.2**

**Draft**

# Document Status

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Version** | **Document Status** | **Author** |
| 02/26/2020 | 1.2 | Draft | May Alaa |

# Document History

|  |  |  |  |
| --- | --- | --- | --- |
| **Version** | **Date** | **Author** | **Change** |
|  |  |  |  |
| 1.0 | 01/24/2020 | Ali Samir | Initial Creation |
| 1.1 | 01/24/2020 | Mohamed M. Farag | Adding initial APIs for components |
| 1.2 | 01/29/2020 | May Alaa | Adding Requirements and APIs |

Contents

[Document Status 2](#_Toc33831406)

[Document History 3](#_Toc33831407)

[Introduction 6](#_Toc33831408)

[1.1 Project Description 6](#_Toc33831409)

[1.2 Block diagram 6](#_Toc33831410)

[Software Context Diagram 7](#_Toc33831411)

[Input Output signals 7](#_Toc33831412)

[Software features 8](#_Toc33831413)

[Static Architecture 9](#_Toc33831414)

[**Requirements:** 11](#_Toc33831415)

Table of figures:

[Figure 1 Block Diagram 7](#_Toc33082078)

# Introduction

## 1.1 Project Description

The Electric Blender System is an appliance created by KENOVO. The electric blender system has 3 speeds that can be configured by the user with high safety to avoid system failure caused by unexpected voltage peaks.

## 1.2 Block diagram





Figure 1 Block Diagram

# Software Context Diagram

# Input Output signals

# Software features

# Static Architecture



# **Requirements:**

**APPLICATION LAYER:**

|  |  |  |  |
| --- | --- | --- | --- |
| **SPEED CONTROL** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_1\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Blender\_Motor\_Init(void); | void | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize the Blender’s motor. |
| Requirement ID | REQ\_PO2EBL\_GDD\_2\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Blender\_Motor\_SetSpeed(uint8\_t Speed); | uint8\_t Speed: Denotes the desired motor speed. | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn the blender’s motor on with desired speed. |
| Requirement ID | REQ\_PO2EBL\_GDD\_3\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Blender\_Motor \_OFF(void); | void | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn the Motor Off. |

|  |  |  |  |
| --- | --- | --- | --- |
| **USER INPUT CONTROLS** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_4\_V01 | | |
| API | Parameters | Return Value | Description |
| Error\_S Speed\_Switch\_Init(void); | void | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize the SPEED\_SWITCH |
| Requirement ID | REQ\_PO2EBL\_GDD\_5\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Speed\_Switch \_Read(void); | void | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall read the SPEED\_SWITCH ‘s Status |

|  |  |  |  |
| --- | --- | --- | --- |
| **POWER PROTECTION** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_6\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Blender\_Voltage\_Init(void); | void | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize the Blender’s voltage sensor |
| Requirement ID | REQ\_PO2EBL\_GDD\_7\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Blender\_Voltage \_Read(void); | void | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall get the Blender’s voltage sensor readings |

|  |  |  |  |
| --- | --- | --- | --- |
| **SPEED INDICATION** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_8\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error Speed\_LED\_Init(void); | void | S\_Error: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize the Speed indication LED. |
| Requirement ID | REQ\_PO2EBL\_GDD\_9\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error Speed\_LED\_ON(void); | void | S\_Error :Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn the Speed indication LED ON. |
| Requirement ID | REQ\_PO2EBL\_GDD\_10\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error Speed\_LED\_OFF(void); | void | S\_Error :Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn the Speed indication LED OFF. |

**ECU ABSTRACTION LAYER:**

|  |  |  |  |
| --- | --- | --- | --- |
| **LED** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_11\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S LED\_Init(u8 Lamp\_Ch\_No); | u8 LED\_Ch\_No: Denotes the Lamp to be initialized | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall initialize a LED given the LED’s channel Number |
| Requirement ID | REQ\_PO2EBL\_GDD\_12\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S LED\_ON(u8 Lamp\_Ch\_No); | u8 LED\_Ch\_No: Denotes the Lamp to be turned on | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn a LED ON given the LED’s channel Number |
| Requirement ID | REQ\_PO2EBL\_GDD\_13\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S LED\_OFF(u8 Lamp\_Ch\_No); | u8 LED\_Ch\_No: Denotes the Lamp to be turned off | Error\_S:Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn a LED Off given the LED’s channel Number |

|  |  |  |  |
| --- | --- | --- | --- |
| **SWITCH** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_14\_V01 | | |
| API | Parameters | Return values | Description |
| Error\_S Switch\_Init(u8 Switch\_Ch\_No); | u8Switch\_Ch\_No: Denotes the Switch to be initialized | Error\_S:Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize a switch given the switch’s channel number |
| Error\_S Switch\_Read(u8 Switch\_Ch\_No); | u8 Switch\_Ch\_No: Denotes the Switch whose status is s to be read | Error\_S:Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall read a switch’s status given the switch’s channel number |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **VOLTAGE SENSOR** |  | |  |  |
| Requirement ID | REQ\_PO2EBL\_GDD\_15\_V01 | | | |
| API | Parameters | | Return Value | Description |
| Error\_S Switch\_Init(u8 Switch\_Ch\_No); | u8Switch\_Ch\_No: Denotes the Switch to be initialized | | Error\_S:Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize a switch given the switch’s channel number |
| Requirement ID | REQ\_PO2EBL\_GDD\_16\_V01 | | | |
| API | Parameters | | Return Value | Description |
| Error\_S Switch\_Read(u8 Switch\_Ch\_No); | u8 Switch\_Ch\_No: Denotes the Switch whose status is s to be read | | Error\_S:Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall read a switch’s status given the switch’s channel number |
| **MOTOR** | | | | |
| Requirement ID | | REQ\_PO2EBL\_GDD\_17\_V01 | | |
| API | | Parameters | Return Value | Description |
| Error\_S Switch\_Init(u8 Switch\_Ch\_No); | | u8Switch\_Ch\_No: Denotes the Switch to be initialized | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall Initialize a switch given the switch’s channel number |
| Requirement ID | | REQ\_PO2EBL\_GDD\_18\_V01 | | |
| API | | Parameters | Return Value | Description |
| Error\_S Motor\_SetSpeed(uint8\_t Motor\_Ch\_No, uint8\_t Motor\_Speed); | | uint8\_t Motor\_Ch\_No: Denotes the motor to be operated.  uint8\_t Motor\_Speed: Denotes the desired motor speed. | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall set the desired motor ‘s speed. |
| Requirement ID | | REQ\_PO2EBL\_GDD\_19\_V01 | | |
| API | | Parameters | Return Value | Description |
| Error\_S Motor\_Off(uint8\_t Motor\_Ch\_No); | | uint8\_t Motor\_Ch\_No: Denotes the motor to be turned off. | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall turn the motor off. |

**MICROCONTROLLER ABSTRACTION LAYER**

|  |  |  |  |
| --- | --- | --- | --- |
| **GPIO** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_20\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error GPIO\_SetPinDir(uint32\_t ui32Port, uint8\_t ui8Pins, uint32\_t ui32PinIO); | uint32\_t ui32Port: Denotes the desired port  uint8\_t ui8Pins: Denotes the desired pin  uint32\_t ui32PinIO: Denotes the Pin mode | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall set pins’ modes |
| Requirement ID | REQ\_PO2EBL\_GDD\_21\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error GPIO\_GetPinVal(uint32\_t ui32Port, uint8\_t ui8Pins); | uint32\_t ui32Port: Denotes the desired port  uint8\_t ui8Pins:Denotes the desired pin | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall read pins’ status |
| Requirement ID | REQ\_PO2EBL\_GDD\_22\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error GPIO\_SetPinVal(uint32\_t ui32Port, uint8\_t ui8Pins, uint8\_t ui8Val); | uint32\_t ui32Port: Denotes the desired port  uint8\_t ui8Pins:Denotes the desired pin  uint8\_t ui8Val: Denotes the desired value. | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall write values to pins |

|  |  |  |  |
| --- | --- | --- | --- |
| **TIMER** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_23\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error TIMER\_Init(uint8\_t Timer\_Ch\_num); | uint8\_t Timer\_Ch\_num: Denotes the desired timer channel  The options can be:  {Timer 0, Timer 1, Timer 2} | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall initialize the timer configurations. |
| Requirement ID | REQ\_PO2EBL\_GDD\_24\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error TIMER\_Start(uint8\_t Timer\_Ch\_num); | uint8\_t Timer\_Ch\_num: Denotes the desired timer channel  The options can be:  {Timer 0, Timer 1, Timer 2} | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall start the desired timer. |
| Requirement ID | REQ\_PO2EBL\_GDD\_25\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error TIMER\_Stop(uint8\_t Timer\_Ch\_num); | uint8\_t Timer\_Ch\_num: Denotes the desired timer channel  The options can be:  {Timer 0, Timer 1, Timer 2} | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall stop the desired timer. |
| Requirement ID | REQ\_PO2EBL\_GDD\_26\_V01 | | |
| API | Parameters | Return values | Description |
| S\_ErrorTIMER\_voidSetCallback(uint8\_t Timer\_Ch\_num , void (\*PFunc)(void)) | uint8\_t Timer\_Ch\_num: Denotes the desired timer channel  The options can be:  {Timer 0, Timer 1, Timer 2}  void (\*PFunc)(void):  void pointer to a callback function. | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall set the desired timer callback. |

|  |  |  |  |
| --- | --- | --- | --- |
| **PWM** | | | |
| Requirement ID | REQ\_PO2EBL\_GDD\_27\_V01 | | |
| API | Parameters | Return Value | Description |
| S\_Error PWM\_Init(uint8\_t PWM\_Ch\_Num); | uint8\_t PWM\_Ch\_Num:Denotes the desired PWM Channel number. | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall initialize the desired PWM channel. |
| Requirement ID | REQ\_PO2EBL\_GDD\_28\_V01 | | |
| API | Parameters | Return values | Description |
| S\_Error PWM\_GenerateSignal(uint8\_t PWM\_Ch\_Num, uint16\_t ONPeriod, uint16\_t TotalPeriod, uint16\_t PeakVoltage\_mV) | uint8\_t PWM\_Ch\_Num:Denotes the desired PWM Channel number.  uint16\_t ONPeriod: Denotes the desired ON period.  uint16\_t TotalPeriod: Denotes uint16\_t PeakVoltage\_mV | Error\_S: Standard Error  OK: If execution happened successfully  NOK: If Execution failed | This API shall generate a PWM signal with the desired duty cycle on the given PWM channel. |